R1150 Safety Data Sheet (SDS)
Safety Data Sheet(SDS / MSDS) Ethylene(Ethene) Ethylene CAS 74-85-1 UN 1962 Class 2.1, flammable gas
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[bookmark: s1]1 Identification of the Substance and Supplier
1.1 Product Identifier

	Item
	Value

	Chinese chemical name
	Ethylene（Ethene）

	English Name
	Ethylene

	—
	R1150, Ethylene(Ethene) Refrigerant

	CAS No.
	74-85-1

	UN No.
	1962 (Ethylene(Ethene), ( ETHYLENE ))

	UN number
	22073

	Transport Hazard Classification
	2.1 class Flammable

	Molecular Formula
	CH₂=CH₂

	Molecular Weight
	28.05 g/mol

	Recommended use
	cascade Ultra-low temperaturesystemLow temperature( -100℃ approx.), gas liquefaction and cryogenic separation, pharmaceutical and biological samplescryogenic.

	supply class
	Industrial grade / Refrigerant grade / High-purity grade(available on request)


1.2 Manufacturer / Supplier Details

	Item
	Value

	Supplier
	Hubei Zhongjin Fluorine Chemical Co., Ltd.

	English Name
	Hubei Zhongjin Fluorine Chemical Co., Ltd.

	Address
	302-3, Beihu Shengying Beihu Office Compound, Qingshan District, Wuhan, Hubei, China

	Postal code
	430080

	Telephone
	15056328442

	Email
	sales@zj-f.com

	Request a quote for
	Contact our sales team for quotations, lead times and third-party test reports.


1.3 Emergency Telephone Number
National chemical emergency hotline: +86-532-83889090 (24 h); supplier emergency telephone: +86 150 5632 8442.
[bookmark: s2]2 Hazards Identification
2.1 GHS Classification

	Hazard Classification
	Description

	Gas under pressure
	Liquefied gas, transported and stored in pressure cylinders or ISO tanks.

	single exposure(Health hazards)
	Inhalation at high concentrations may cause central nervous system depression (narcotic effects) with dizziness, drowsiness and headache; very high concentrations may cause cardiac arrhythmia.

	Flammable gas (where applicable)
	ASHRAE Safety classification A3 (Low, Flammable), Spillage confined space flammable mixture.


Note: frostbite from liquid contact with skin or eyes is a physical cryogenic injury; GHS has no separate frostbite hazard class.
2.2 GHS Label Elements
GHS02Flame Flammable
GHS04steel cylinderGas under pressure

	Item
	Value

	Signal Word
	Danger

	Pictogram
	Flame, steel cylinder


Hazard Statements (H-codes)
H220 Extremely flammable gas.
H280 Contains gas under pressure; may explode if heated.
H336 May cause drowsiness or dizziness.
Precautionary Statements (P-codes)
P202 Do not handle in enclosed or poorly ventilated areas.
P210 Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.
P233 Keep container tightly closed.
P271 Use only outdoors or in a well-ventilated area.
P304+P340 IF INHALED: Remove person to fresh air and keep comfortable for breathing.
P377 Do not use water to extinguish a leaking gas fire.
P381 In case of leakage, eliminate all ignition sources.
P403 Store in a well-ventilated place.
2.3 Other Hazards
Extremely flammable gas, Explosive limitsapprox. 2.7%～36%,.
Minimum ignition energyapprox. 0.07 mJ, Extremely flammable,.
Critical TemperatureLow(approx. 9.2℃), steel cylinder.
ODP = 0, GWP approx. 4, cryogenicsystem refrigerant.
[bookmark: s3]3 Composition / Information on Ingredients
3.1 Substance / Mixture
this product.
3.2 Composition Information

	Component
	CAS No.
	Concentration (mass fraction)

	Ethylene(Ethene)( R1150 )
	74-85-1
	≥ 99.5% (Premium Grade ≥ 99.9% )


3.3 Impurity Information

	Impurity
	Premium Grade
	First Grade

	Acidity( HCl )
	≤ 0.1 ppm
	≤ 1 ppm

	Moisture
	≤ 5 ppm
	≤ 10 ppm

	Evaporation Residue
	≤ 50 ppm
	≤ 100 ppm

	Non-Condensable Gas( 25 ℃, )
	≤ 1.5 %
	≤ 1.5 %

	Chloride test
	Pass
	Pass


[bookmark: s4]4 First-Aid Measures
4.1 Description of First-Aid Measures
General advice:,. doctor Description.
Inhalation
fresh air,.
If breathing is difficult, administer oxygen.
( or, ).
(CPR).
Keep the patient warm and at rest, monitor closely and seek medical attention if needed.
Skin contact (frostbite)
(37～40 ℃)frostbite Body Part,.
(>40 ℃) or (, ).
frostbite Body Part,.
and,,.
Cover the affected area with a sterile dressing and seek immediate medical attention.
Eye contact
or 15.
Body Part.
Remove contact lenses before rinsing, if present and easy to do.
doctor.
Ingestion
Not applicable. or, Ingestion.
Spillage or emissions, ignition sources,.
4.2 Most Important Symptoms and Health Effects
Inhalation: dizziness, drowsiness, headache,,; and cardiac arrhythmia.
Skin contact: frostbite(,,, ).
Eye contact: frostbite,,.
decomposition products Inhalation: and;refrigerant decomposition products.
4.3 Notes to Physician
Treat symptomatically, keep the airway clear and give oxygen if needed.
cardiac arrhythmia.
class(, ).
frostbiteperfrostbite, 37～40 ℃, or.
decomposition products(, ),,.
[bookmark: s5]5 Fire-Fighting Measures
5.1 Suitable Extinguishing Media
Extremely flammable gas,, carbon dioxide, Firefighting. Firefighting;, Vapour.
5.2 Specific Hazards Arising from the Substance
steel cylinder,; or,.
Value.
and, High temperature or.
5.3 Hazardous Combustion Products
High temperaturedecomposition products: carbon monoxide(CO).
5.4 Advice for Firefighters
Self-contained breathing apparatus(SCBA),.
Move containers from the fire area to open ground if safe to do so.
Firefighting.
Isolate the area and keep unauthorized personnel out.
Spillage Liquefied gas,.
[bookmark: s6]6 Accidental Release Measures
6.1 Personal Precautions and Protective Equipment
Spillage,,.
(SCBA),, Low temperatureprotective gloves.
Approach from upwind.
Spillage.
or Spillage.
Assign an emergency liaison and arrange external support.
6.2 Environmental Precautions
or enclosed.
Ventilate the area to disperse the gas.
Spillageemissions, recovery.
Avoid release to air, water and soil.
6.3 Methods and Materials for Containment and Clean-Up
eliminate all ignition sources. Spillage, Vapourlow-lying areas and Other Flammable. Spillage. recoveryrecovery.
steel cylinder Spillage, steel cylinder, or Supplier.
If recovery is not possible, dilute with water spray while preventing water contamination.
6.4 Reference
8 (Exposure controls / personal protection) 13 (Disposal).
Special warning:Vapourlow-lying areasenclosedoxygen deficiency. enclosed or low-lying areasoxygen(≥ 19.5%),.
[bookmark: s7]7 Handling and Storage
7.1 Precautions for Safe Handling
enclosed, ventilation or.
Operators must be trained, follow procedures and hold the required certification.
Spillage.
and, oxygen.
steel cylinder,,,,.
Accidental release measures equipment.
No smoking, eating or drinking in the workplace.
frostbite.
steel cylinder, tightness.
Flammable refrigerant, Spillage and, recovery.
7.2 Conditions for Safe Storage, including Incompatibilities
Storage,, ventilation, 40 ℃, ignition source, heat source and.
steel cylinder, and,,, and.
and oxygen, and (,, )Flammable,.
and, Low 0.05 MPa.
Accidental release measures equipment,.
Apply two-person receiving and custody control.
Filling Ratio: ≤ 0.4 kg/L.
Flammable and explosion-proofventilation, equipmentperexplosion-proof.
sparks equipment.
7.3 Specific End Use(s)
use,. ODP, GWP Low, "Montreal Protocol" and "Kigali Amendment"controlled.
[bookmark: s8]8 Exposure Controls / Personal Protection
8.1 Occupational Exposure Limits
ACGIH TLV-TWA, asphyxiation.
Prepared in accordance with GBZ 2.1-2019"Occupational exposure limits 1: ", Occupational exposure limits,.
8.2 Monitoring Methods
Gas chromatography(GC-FID or GC-MS);;.
8.3 Engineering Controls
enclosed, ventilation or.
Provide safety showers and eyewash stations.
Spillage.
Use explosion-proof electrical equipment.
8.4 Personal Protective Equipment

	Body Part
	Protection Required

	Respiratory protection
	(Low)Protection;Higher(Vapour / ); or, Self-contained breathing apparatus( SCBA ).

	Eye protection
	Protection; or Protection or /, frostbite.

	Protection
	protective gloves;Low temperature(, ).

	Protection
	Wear standard work clothing; wear cold-protective clothing when handling liquid.

	Other
	Inhalation at high concentrations;, or Other.


8.5 Hygiene Measures
Remove contaminated clothing and wash skin after work.
Maintain good personal hygiene.
Provide eyewash stations and emergency showers at the workplace.
[bookmark: s9]9 Physical and Chemical Properties
9.1 Basic Physical and Chemical Properties

	Item
	Typical Value

	Appearance
	Colorless, transparent liquefied gas

	Odor
	Faint sweet odour

	Boiling point( 101.3 kPa )
	-103.7 ℃

	Freezing Point
	-169.2 ℃

	Critical Temperature
	9.2 ℃

	Critical Pressure
	5.04 MPa

	Critical Density
	approx. 214 kg/m³

	Vapor Pressure( 25 ℃, )
	approx. 6.3 MPa (Critical Temperature, )

	Latent Heat of Vaporization (at boiling point)
	approx. 482 kJ/kg

	Vapor Specific Heat( 25 ℃, 101.3 kPa )
	approx. 1.53 kJ/(kg K)

	Vapor Thermal Conductivity( 25 ℃ )
	approx. 0.0208 W/(m K)

	Vapor Viscosity( 25 ℃ )
	approx. 0.0103 mPa s

	Water Solubility( 25 ℃ )
	Slightly soluble

	Auto-Ignition Temperature
	425 ℃

	Flammability Limits in Air (vol.%)
	2.7 % ~ 36 %

	Minimum ignition energy
	approx. 0.07 mJ

	Occupational exposure limits OEL ( 8 h TWA )
	200 ppm (per Ethylene(Ethene)data)

	Ozone depletion potential (ODP) ODP
	0

	Global warming potential (GWP) GWP ( 100 years)
	approx. 4

	Atmospheric Lifetime
	approx. 1.9

	ASHRAE Safety classification
	A3 (Low, Flammable)

	UN Transport
	Ethylene(Ethene), ( ETHYLENE )

	UN number( CN )
	22073


9.2 Other Safety Data

	Item
	Value

	ASHRAE Safety classification
	A3 (Low, Flammable)

	Atmospheric Lifetime
	approx. 2.5 years

	Atmospheric Lifetime
	per IPCC, and OH.

	Decomposition temperature
	> 250 ℃ (controlled High temperature).


[bookmark: s10]10 Stability and Reactivity
10.1 Reactivity
Chemically stable at ambient temperature and pressure.
10.2 Chemical Stability
Stable under normal temperature and pressure.
10.3 Possibility of Hazardous Reactions
High temperature(> 250 ℃), carbon monoxide(CO).
and, High temperature or.
and oxygenoxygen.
10.4 Conditions to Avoid
High temperature, open flames, heat source, steel cylinder,.
10.5 Incompatible Materials
(,,,, ), oxygen.
10.6 Hazardous Decomposition Products
carbon monoxide(CO), Other /.
10.7 Hazardous Polymerization
No polymerisation occurs.
[bookmark: s11]11 Toxicological Information
11.1 Acute Toxicity
Inhalation LC50(4 hours)approx. 10,000 ppm;oxygen deficiency and.
11.2 Skin Corrosion / Irritation
frostbite,. GHS class: Skin corrosion / class(frostbite).
11.3 Serious Eye Damage / Irritation
frostbite.
11.4 Respiratory or Skin Sensitization
. testingdata.
11.5 Germ Cell Mutagenicity
testing(Ames testing, testing, testing).
11.6 Carcinogenicity
Carcinogenicity. IARC;ACGIH A4 class( class class);EPA D ( class class).
11.7 Reproductive Toxicity
testing Reproductive toxicity, class Reproductive toxicitydata.
11.8 STOT - Single Exposure
narcotic effects(Category 3): Inhalation at high concentrations central nervous system depression, dizziness, drowsiness, headache,.
cardiac arrhythmia, or.
11.9 STOT - Repeated Exposure
Low. Inhalationtesting.
11.10 Aspiration Hazard
Inhalation, Inhalation at high concentrations central nervous system depression. decomposition products(, ).
[bookmark: s12]12 Ecological Information
12.1 Ecotoxicity

	Test Species
	Endpoint & Result

	class Acute toxicity
	96 h LC50 > 100 mg/L ( classLow)

	class Acute toxicity
	48 h EC50 > 100 mg/L

	class
	72 h EC50 > 100 mg/L


12.2 Persistence and Degradability
Main and, Atmospheric Lifetimeapprox. approx. 2.5 years.
Biodegradability: not readily biodegradable.
Hydrolysis: not readily hydrolysed at ambient temperature.
12.3 Bioaccumulative Potential
log P Low, Low(Low log P = 4.5).
12.4 Mobility in Soil
Water SolubilityLow,..
12.5 PBT and vPvB Assessment
PBT(Persistence, bioaccumulation and toxicity)/ vPvB(Very persistent and very bioaccumulative).
12.6 Other Adverse Environmental Effects
Ozone depletion potential (ODP)(ODP): 0(Relative CFC-11 = 1).
Global warming potential (GWP)(GWP, 100 years): approx. 4(Relative CO₂ = 1).
Large releases affect the ozone layer and global warming; strictly control emissions and prioritise recovery.
[bookmark: s13]13 Disposal Considerations
13.1 Waste Treatment Methods

	Waste Type
	Disposal Method

	—
	emissions. recovery,;recovery Danger;High temperature,., or.

	Packaging
	steel cylinder Supplier or, or;steel cylinder, per Danger.


13.2 Disposal Precautions
Regulations, "".
Protection( 8 ).
Ensure adequate ventilation to prevent asphyxiation.
Disposal,.
[bookmark: s14]14 Transport Information
14.1 UN Number
1962(Ethylene(Ethene), (ETHYLENE))
14.2 UN Proper Shipping Name

	Item
	Value

	Chinese
	Ethylene(Ethene)

	English
	ETHYLENE


14.3 Transport Hazard Class
Class 2.1, flammable gas
14.4 Packing Group
Not applicable( 2 class Packing group).
14.5 Transport Labels
Main Hazard: Flammable.
Hazard:.
14.6 Packaging Method
(steel cylinder), steel cylinder GB 5099"".
Packaging: 20kg, 50kg explosion-proofsteel cylinder, 400kg steel cylinder, ISO ISO tank.
Filling Ratio: ≤ 0.4 kg/L.
steel cylinder Storage and Transport,.
14.7 Special Precautions by Transport Mode

	Transport Mode
	Special Requirements

	Transport( GB/T 12268 )
	Transport DangerTransport;steel cylinder;steel cylinder,,;Transport,;per,.

	Transport(Danger Transport)
	Transport, steel cylinder or.

	Transport( IMDG )
	UN 1962, 2.1 class Flammable;Marine pollutant:; class: A ( or ).

	Transport( ICAO/IATA DGR )
	UN 1962, 2.1 class Flammable; / Transport(Packaging).


14.8 Transport Precautions
and oxygen,,.
Transport Accidental release measures equipment.
Transport,.
Transport,, High temperature.
Keep away from ignition sources, heat and high-temperature areas during stops.
Vehicles must be fitted with exhaust flame arresters.
steel cylinder.
[bookmark: s15]15 Regulatory Information
15.1 Chinese Regulations
Regulations on the Safety Management of Hazardous Chemicals (State Council Decree No. 591)
Catalogue of Hazardous Chemicals (2015 edition): listed
GB 30000 series: GHS classification and labelling
GB/T 16483-2008: SDS preparation standard
GBZ 2.1-2019: occupational exposure limits for chemical agents
""(TSG 23-2021)
"Danger Transport": Danger Transport
Air Pollution Prevention and Control Law of the PRC: greenhouse gas controls
"": and Danger
GHS( class) 8
Not a controlled ozone-depleting substance
Not listed under the Kigali Amendment
15.2 International Regulations
EU REACH Regulations(EC 1907/2006) and CLP Regulations(EC 1272/2008)
EU F-Gas Regulations(EC 517/2014): control
EPA SNAP / OSHA HCS 2012 / DOT 49 CFR
ADR/RID /Danger Transport;IMDG Code;IATA DGR Transport
[bookmark: s16]16 Other Information
16.1 References
NIOSH Pocket Guide to Chemical Hazards
International Chemical Safety Card (ICSC)
NOAA CAMEO Chemicals Database
PubChem Compound Database
ASHRAE Handbook — Refrigeration Systems and Applications
GB/T 16483-2008"Description Value Item"
GB 30000 " class"
"Montreal Protocol"Kigali Amendmentapprox.
16.2 Abbreviations and Acronyms

	Abbreviation
	Full Name

	SDS / MSDS
	Description / Description

	GHS
	class

	CAS
	(No.)

	UN
	(UN number)

	ODP
	Ozone depletion potential (ODP)

	GWP
	Global warming potential (GWP)

	LC50
	LC50

	LD50
	LD50

	TLV-TWA
	See the Safety Data Sheet (SDS) for details.

	PEL
	Permissible exposure limit

	SCBA
	Self-contained breathing apparatus

	PBT
	Persistence, bioaccumulation and toxicity

	vPvB
	Very persistent and very bioaccumulative

	HCFC
	HCFC

	ODS
	Ozone-depleting substance

	HFO
	HFO

	A2L
	Low, Flammable( ASHRAE 34 / ISO 817 )

	A3
	Low, Flammable( ASHRAE 34 / ISO 817 )


16.3 Disclaimer
Safety Data Sheet (SDS) GB/T 16483-2008 GHS Prepared by,,., Specification or. Regulations, Protection. Description or, Prepared by. data Regulations,.
Prepared by: | Reviewed by: | Approved by: | Hubei Zhongjin Fluorine Chemical Co., Ltd.
Get R1150 Technical Data Sheet & Quotation
SDS R1150 Prepared in accordance with., Specification(TDS) or Batch, or sales team.
Specification TDS Request a quote for and
Hubei Zhongjin Fluorine Chemical Co., Ltd.: 2026-10-20Description Prepared in accordance with GB/T 16483-2008"Description Value Item"Prepared by, data Typical,;.





