R152a Refrigerant Specification
Technical Data Sheet（TDS）
Hubei Zhongjin Fluorine Chemical Co., Ltd. ｜ No. ZJ-TDS-R152A-2026 ｜ V1.0
1. R152a, and
1. data Typical,.
1. Prepared by: Reviewed by: Approved by
	Item
	Value

	—
	ZJ-TDS-R152A-2026

	Version
	V1.0

	Issue date
	2026-10-20

	—
	2027-10-20

	Applicable Standard
	Q/ZJ 033-2026 (Safety classification GB/T 7778, ASHRAE 34 / ISO 817 )

	Prepared by / Reviewed by / Approved by
	See the Safety Data Sheet (SDS) for details.

	—
	Hubei Zhongjin Fluorine Chemical Co., Ltd.



1 Product Identification
	Item
	Value

	Product Name
	R152a Refrigerant

	Chemical Name
	1,1- Fluoroethane(Refrigerant R 161)

	English Name
	1,1-Difluoroethane （ Refrigerant R 152a ）

	Molecular Formula
	CH₃CHF₂

	Molecular Weight
	66.04

	CAS Registry number
	75-37-6

	No.( UN )
	1030

	Transport Hazard Class
	2.1 class Flammable

	ASHRAE Safety classification
	A2 (Low toxicity, flammable)

	Applicable Standard
	Q/ZJ 033-2026



2 Physical & Chemical Properties
R152a Typicaldata, system and,.
	Item
	Typical Value

	Appearance
	Colorless, transparent liquefied gas

	Odor
	Slight ethereal odour

	Boiling point( 101.3 kPa )
	-25.0 ℃

	Freezing Point
	-138.8 ℃

	Critical Temperature
	approx. 113.3 ℃

	Critical Pressure
	approx. 4.56 MPa

	Vapor Pressure( 25 ℃, )
	approx. 1.08 MPa

	Liquid Density( 25 ℃ )
	approx. 948 kg/m³

	Saturated Vapor Density( 25 ℃ )
	approx. 25.8 kg/m³

	Latent Heat of Vaporization (at boiling point)
	approx. 246 kJ/kg

	Liquid Specific Heat( 25 ℃ )
	approx. 1.42 kJ/(kg K)

	Vapor Specific Heat( 25 ℃, 101.3 kPa )
	approx. 0.85 kJ/(kg K)

	Water Solubility( 25 ℃ )
	Slightly soluble

	Auto-Ignition Temperature
	approx. 470 ℃

	Flammability Limits in Air (vol.%)
	1.5 % ~ 9.5 %

	Minimum ignition energy
	approx. 0.25 mJ

	Occupational exposure limits OEL ( 8 h TWA )
	1000 ppm (per R152a data)

	Ozone depletion potential (ODP) ODP
	0

	Global warming potential (GWP) GWP ( 100 years)
	approx. 148

	Atmospheric Lifetime
	approx. 12



3 Quality Specifications & Test Methods
R152a Parameter, Batch COA.
	Item
	Parameter
	Test Method

	Appearance
	Colourless and clear, free of suspended matter and mechanical impurities
	Visual inspection

	Purity
	≥ 99.80 %
	Gas chromatography GC-FID

	Moisture
	≤ 20 ppm
	—

	Acidity( HCl )
	≤ 0.1 ppm
	—

	Evaporation Residue
	≤ 0.01 %
	Gravimetric method

	Non-Condensable Gas
	≤ 1.5 %
	Gas chromatography

	( Cl⁻ )
	Negative (pass)
	Silver nitrate turbidimetry



4 Comparison with Common Refrigerants
	Comparison Item
	R152a (this product)
	R32
	R134a

	Composition
	Single compound CH₃CHF₂
	Single compound CH₂F₂
	Single compound CH₂FCF₃

	Boiling point
	-25.0 ℃
	-51.7 ℃
	-26.3 ℃

	Critical Temperature
	approx. 113.3 ℃
	78.1 ℃
	101.1 ℃

	ODP
	0
	0
	0

	GWP ( 100 years)
	approx. 148
	675
	approx. 1,430

	ASHRAE Safety classification
	A2 (Flammable)
	A2L (Mildly flammable)
	A1 (Non-flammable)

	Flammability limits in air
	1.5 % ~ 9.5 %
	13.5 % ~ 27.5 %
	Non-flammable

	Relative charge
	approx. R134a 60 %
	approx. R134a 70 %
	Baseline 100 %

	Main
	Low GWP
	Single compound and
	refrigerant

	Current selection
	—
	residential air conditioning refrigerant
	Subject to quota phase-down



5 Packaging Specifications
	Package Type
	Specification
	Filling Ratio
	Valve Connection
	Application

	disposable cylinder
	50 kg (customizable 30 kg )
	≤ 0.90 kg/L
	W21.8-14 / CGA (perorder)
	and testingquantity

	steel cylinder
	400 kg
	≤ 0.90 kg/L
	W21.8-14
	Item and supply

	cylinder pallet
	Made to order
	Per cylinder
	W21.8-14
	Itemdistribution

	ISO ISO tank
	Made to order
	per ISO tank
	ISO tankconnection
	Transport



Filling Ratioper"", steel cylinderper.
6 Applications
(1)Typicalapplication
low-GWP Refrigerant
air conditioninglow-GWP Alternatives
commercial refrigeration and heat pump
R449A / R454B / R516A supply
(2)Equipment Compatibility & Charging Advice
1. R152a A2 Flammable refrigerant, systemperexplosion-proof: explosion-proof,, ventilation and Flammable.
1. R152a Main,;refrigerantcompressor.
1. per, and.
1. and, POE;system, and and refrigerant.
1. and serviceexplosion-proofcharging, recovery and leak detection equipment, recoverynitrogen,.
7 Storage & Transport
1. Storage,, ventilation, 40 ℃, ignition source, heat source and.
1. steel cylinder, and,,, and.
1. 2.1 class Flammable, perexplosion-proof equipment, Flammable and explosion-proofventilation.
1. and oxygen,, Flammable, explosion-proof and.
1. and, Low 0.05 MPa.
1. Transportper Danger 2.1 class, Firefighting and, and.
8 Safety & Handling
<b>Flammability and explosion risk</b>: R152a A2 Flammable refrigerant, Explosive limits 1.5 % ~ 9.5 %, Low, explosion-proof, ventilation.
<b>Spillage</b>: ignition sourceventilation,;explosion-proof and;explosion-proofleak detection.
<b>Firefighting</b>:; or carbon dioxide Firefighting, steel cylinder. Spillage Flame,.
<b>frostbite Protection</b>: Liquefied gasfrostbite, and;frostbite 40 ℃.
<b>Inhalation and </b>: Vapourasphyxiation, and, fresh airoxygen;Eye contact 15.
<b></b>: High temperature and, and.
9 Quality Assurance & Shipping Documents
1. Batch COA, Purity( or ), Moisture, Acidity and Evaporation Residue.
1. Moisture, and Low temperature.
1. 12 months, Batch, No. and.
1. perthird-party test report(SGS / ), SDS Description REACH, RoHS.
10 Frequently Asked Questions
R152a What is it, and why？: R152a(1,1-Difluoroethane(Refrigerant R 152a), CH₃CHF₂) HFC class refrigerant, ODP, GWP approx. 148. Boiling point -25 ℃, A2 Flammable, 1.5 %, Main--R449A, R454B, R516A low-GWP refrigerantLowFlammable and.

R152a GWP approx. 148 What does it imply?: low-GWP refrigerant. R449A, R454B, R516A class Refrigerant, R152a Temperature glide and LowRisk, low-GWP and A1/A2L Safety class.

R152a ？: R152a "Kigali Amendment"control HFC,, and quota, Procurement Supplier quota and use. Refrigerant and, Procurement.

Disclaimer
Specificationdata Typical,;Parameter Batch COA. and, or or, equipment and Regulations.
Hubei Zhongjin Fluorine Chemical Co., Ltd.: 2026-10-20




